#### TECHNICAL SPECIFICATION FORM

**Tender No. 91188415**

Suppliers are requested to complete this form, sign it and return it as part of their bid submission. Suppliers should fill out this form in accordance with the instructions indicated. No alterations to its format shall be permitted and no substitutions shall be accepted.

This Technical Specification Form has an integral part with the Bid Price Form for this tender.

**Supplier Name:**

**Quotation No:**

**Tender purpose: Procurement of Equipment for Crop Doctors**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **No.** | **Requirements/Specifications** | **Confirmation of Compliance to the Specification**  (YES or NO).  **If NO, please explain** | **Proposed Brand Type & Specification**  *(please mention the detailed specifications and* Picture/Brochure/Catalog/Link/ etc.) | **Picture**  **(as sample, not mandatory brand)** |
| **1** | **Pruning Shears**   * High-quality pruning shear for exact shaping and precise cutting results * Size: 8“(overall length 200-220 mm) * Material: blade is made from carbon steel anti-rust/stainless steel; Handle is full aluminium with rubber (non-slip treatment); it has a lock system; and can be used to cut the branches with max diameter: 15 mm |  | ***Note:*** *Supplier is not allowed to quote more than one item (options) with different prices for one kind of item requested. Suppliers who do not comply will be ruled out from the tender evaluation.*  ***Catatan:*** *Pesera tender tidak diijinkan untuk memberikan penawaran lebih dari satu jenis (pilihan) dengan harga yang berbeda untuk setiap item yang diminta.*  *Peserta tender yang tidak mematuhi hal di atas, tidak akan diikut sertakan dalam proses evaluasi.*  *The specification proposed should be clear, detailed (brand/type/detailed specs) and not ambiguous. This is a very important part of the evaluation process.* |  |
| **2** | **Pruning Saw**   * High Quality Pruning Saw that can be used to cut large tree branches and limbs * Size: Curve Blade with length (mm): 250 – 310 mm,  Overall Length (mm): 450-480 mm * Material: blade made of stainless steel/high carbon steel (never need resharpening); Comfortable handle (non-slip) |  |  |  |
| **3** | **Soil pH and Moisture Tester**   * Measuring device that can be used to measure soil acidity and soil moisture by inserting it directly into the soil * Reading display using an Analogue pointer needle; Measurement Range: 3 ~ 8 pH * Resolution: 0.2 pH * Humidity Range: 8/WET – 1/DRY |  |  |  |
| **4** | **Grafting Knife**   * Grafting knife that can be used to inoculate plants. Sharp and sturdy folding knife, folded forwards or backwards. Two blades, long and short * The grafting knife should be multifunctional knife, not only limited to grafting purposes but can be used for various other purposes, lightweight, comfortable to use * Size: Short blade length: 4.5 cm; Long blade length size: 6 cm; with total open blade length: 195 mm; and total closed blade length: 100 mm * Material: Blade made of stainless steel, handle is made of plastic. |  |  |  |
| **5** | **Rain gauge Ombrometer**   * Analogue device to measure rain fall * Rain Gauge Ombrometer, completed Measuring Glass Unit; both following BMKG standards * Material: made from stainless steel * Ring funnel, funnel pipe, body pipe made of brass * Body made of good quality stainless steel with a minimum thickness of 0.4 mm * Funnel area: 100 cm2 * Height: 60 cm * At the bottom of the measuring body there is a water faucet (to be measured), and the faucet can be replaced easily in case of damage |  |  |  |
| **6** | **Drawstring Backpack (with printed logos)**   * Comfortable backpack for use by farmers (with shoulder pads or other applications that increase comfort, please specify in your offer). It will be used to bring the tools such as pruning scissors, pruning saw, coffee GAP handbook (A4 format), and grafting knife * Logos of the project partners should be printed well visibly on it (GIZ, Kementan, Dinas Pertanian Bandung and Indocafco; digital logo files will be provided). * Material: high-quality, water-resistant, durable polyester fabrics * Capacity: large compartment measures 30 cm x 40 cm (length x height), big enough for pruning saw, pruning shears, and books or daily supplies (e.g. water bottle). |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **TERMS AND CONDITIONS** | | **Please**  ***tick* *“*Yes*”* or *”*No”** | | **Remarks** |
| 1 | Delivery date after PO released (**please state number of days**) and delivery plan/schedule  Delivery address:  Kampung Gambung RT 04 RW 08,  Desa Mekarsari, Kec. Pasir Jambu,  Kab. Bandung, Jawa Barat 40972 |  | | ------- days  Delivery plan: |
| 2 | The Supplier must deliver the goods within 30 days after signing the PO to the delivery address as mentioned above. |  YES |  NO |  |
| 3 | Validity of Quotation is 30 calendar days |  YES |  NO |  |
| 4 | The items proposed are new and original. Please provide photos/ pictures. |  YES |  NO |  |
| 5 | The Supplier should be responsible for the packing |  YES |  NO |  |
| 6 | Warranty: The Supplier must replace broken equipment  The condition of the equipment will be checked within 3 days after arrival at the delivery address. Rejected items shall be replaced within 2 weeks. |  YES |  NO |  |
| 7 | The quality inspection shall be conducted when the goods are delivered. Any defects shall be remedied by the Supplier without any delay |  YES |  NO |  |
| 8 | Payment terms 30 days after receipt of the Supplier's invoice and delivery of the goods specified in the Purchase Order |  YES |  NO |  |
| 9 | All prices/rates quoted must be exclusive of all taxes since GIZ including its subsidiary organs is exempt from taxes according to PMK No. 215/PMK 03/2008 and KMK No. 17/KMK 010/Year 2021.  GIZ shall process the VAT with tax exemption to BADORA. The process of tax exemption will take 2 - 3 months.  The Supplier is obliged to release the Tax Invoice with code 08 (tax exemption). Please provide the PKP and/ PTKP Letter. |  YES |  NO |  |
| 10 | Supplier Self-Declaration to determine the origin or source of the goods offered shall be signed and attached with the tender document (obligatory) – Annex 3  **(Harus di tandatangani dan di lampirkan pada saat submit penawaran)** |  YES |  NO |  |
| 11 | Declaration of Prevention of Terrorism shall be signed and attached with the tender document – Annex 4  (**Harus di tandatangani dan di lampirkan pada saat submit penawaran** |  YES |  NO |  |

I, the undersigned, certify that I am duly authorized by [*supplier name]* to sign this quotation and bind [*supplier name*] should GIZ accept this quotation:

Contact Person: *name*

Telp/Hp:

Job title:

Date:

Signature and company stamp: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

|  |
| --- |
|  |