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A. TECHNICAL SPECIFICATIONS AND PRICING LIST


	No
	Item
	Description 
	Quantity 
	UNIT PRICE (IQD) 
	Reference Picture

	1
	Diesel Fuel
	Diesel Fuel, density @15C(0.825-0.840). flash point C (60-75), Sulphur <1000 to be used for generators and big machines
	64,000 L
	 
	



B. DELIVERY										

· The requested item should Be delivered to presidential Square, Jadriyah, Baghdad, Iraq.
· The item needs to be delivered within 48 hours after receiving the purchase order.									
C. REMARKS and CONDITION
· Fuel Quantity will be based on need/demand and shall be between (and not limited to) 4,000L – 8,000L per request.
· quality of the fuel should remain constant as it is checked and accepted by the Facility manager.			
· Supplying, loading, offloading, and transportation are included.
· The bidders are required to provide test laboratory results that comply with the fuel specification required.
· The quality of the fuel should remain constant as it is checked and accepted by GIZ Focal Point.
· The supplier MUST provide evidence of having successfully completed at least three similar supplies within the city in the past five years. Acceptable evidence includes completion certificates, reference letters from clients, or contracts mentioning the amount/quantities of the fuel supplies.
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